:INPut:ANALog:COUPling:PAIRed | command/query

Gets or sets a value indicating whether input parameters of paired channels (input channels that are part of the same logical channel, like I+jQ) are coupled.

Command Syntax: | :INPut:ANALog:COUPling:PAIRed <isCoupled>
<isCoupled> | ::= | 0 | 1
Query Syntax: | :INPut:ANALog:COUPling:PAIRed?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :INP:ANAL:COUP:PAIR 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Analog.IsCouplePairedChannels

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |