[:SENSe]:WCDMa[:FORMat]:DLINk:SYNC:ANTenna:TWO:MODE | command/query

Gets or sets the synchronization mode used for Antenna-2 in downlink MIMO measurements.

Command Syntax: | [:SENSe]:WCDMa[:FORMat]:DLINk:SYNC:ANTenna:TWO:MODE <value>
<value> | ::= | "Cpich" | "Sch" | "Antenna2Cpich" | "Symbol"
Query Syntax: | [:SENSe]:WCDMa[:FORMat]:DLINk:SYNC:ANTenna:TWO:MODE?
Returns | ::= | "Cpich" | "Sch" | "Antenna2Cpich" | "Symbol"
Remarks: | <none>
Example: |
    :WCDM:DLIN:SYNC:ANT:TWO:MODE "Cpich"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.Antenna2DownlinkSynchronizationMode Agilent.SA.Vsa.Wcdma.DownlinkSynchronizationMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |