:TRACe:MARKer:BANDwidth:ENABled | command/query

Gets or sets a value indicating whether the band power calculation is enabled for this marker.

Command Syntax: | :TRACe[1:N]:MARKer[1:N]:BANDwidth:ENABled <isVisible>
<isVisible> | ::= | 0 | 1
Query Syntax: | :TRACe[1:N]:MARKer[1:N]:BANDwidth:ENABled?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TRAC:MARK:BAND:ENAB 0
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Marker.IsBandVisible

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |