:MEASure:CONFigure | command/query

Sets or gets the active measurement type.

Command Syntax: | :MEASure:CONFigure <measName>
<measName> | ::= | VECTor | ADEMod | DDEMod | GSM | CUSTomofdm | RFID | LTE | C2K | TDSCdma | EVDO | WCDMa | W16D | W16E | W11A | W11B | W11N | MBOFdm | TEDS
Query Syntax: | :MEASure:CONFigure?
Returns | ::= | VECTor | ADEMod | DDEMod | GSM | CUSTomofdm | RFID | LTE | C2K | TDSCdma | EVDO | WCDMa | W16D | W16E | W11A | W11B | W11N | MBOFdm | TEDS
Remarks: | This command accepts a single enumeration argument with any of the following values:
    VECTor
    ADEMod
    DDEMod
    GSM
    CUSTomofdm
    RFID
    LTE
    C2K
    TDSCdma
    EVDO
    WCDMa
    W16D
    W16E
    W11A
    W11B
    W11N
    MBOFdm
    TEDS       (added in SCPI version 16.00)
The command accepts the short or long form. The query returns only the short form (uppercase).
Example: |
    :MEAS:CONF CUST     //Switches to Custom OFDM
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Measurement.SetMeasurementExtension(Type)

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |