[:SENSe]:LTE[:FORMat]:DLINk:ANTenna:SYNC:PORT | command/query

Gets or sets the P-SS/S-SS Antenna Port or Ports used for synchronization signal transmission.

Command Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:ANTenna:SYNC:PORT <value>
<value> | ::= | "Port0" | "Port1" | "Port2" | "Port3" | "All"
Query Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:ANTenna:SYNC:PORT?
Returns | ::= | "Port0" | "Port1" | "Port2" | "Port3" | "All"
Remarks: | <none>
Example: |
    :LTE:DLIN:ANT:SYNC:PORT "Port0"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.SynchronizationSignalAntennaPort Agilent.SA.Vsa.Lte.SynchronizationSignalAntennaPortType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |