[:SENSe]:LTE:PROFile:MBSFn:ACTive | command/query

Gets or sets a value indicating whether the signal has an MBSFN region

Command Syntax: | [:SENSe]:LTE:PROFile:MBSFn:ACTive <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:MBSFn:ACTive?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:PROF:MBSF:ACT 0
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.IsMbsfnActive

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |