[:SENSe]:LTE[:FORMat]:DLINk:INPut:REFerence[:CHANnel] | command/query

Gets or sets the reference measurement input channel.

Command Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:INPut:REFerence[:CHANnel] <value>
<value> | ::= | "Channel1" | "Channel2" | "Channel3" | "Channel4" | "Channel5" | "Channel6" | "Channel7" | "Channel8"
Query Syntax: | [:SENSe]:LTE[:FORMat]:DLINk:INPut:REFerence[:CHANnel]?
Returns | ::= | "Channel1" | "Channel2" | "Channel3" | "Channel4" | "Channel5" | "Channel6" | "Channel7" | "Channel8"
Remarks: | <none>
Example: |
    :LTE:DLIN:INP:REF "Channel1"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.InputChannel Agilent.SA.Vsa.Lte.InputChannelType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |