[:SENSe]:CORRection:ECONverter:IFCenter | command/query

Gets or sets the center frequency at the IF output of the external frequency converter.

Command Syntax: | [:SENSe]:CORRection[1:N]:ECONverter:IFCenter <center>
<center> | ::= | Real number
Query Syntax: | [:SENSe]:CORRection[1:N]:ECONverter:IFCenter?
Returns | ::= | Real number
Remarks: | <none>
Version: | 16.20 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Correction.ExternalConverterIFCenter

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |