[:SENSe]:DDEMod[:FORMat]:PRESet | command

Set the digital demodulation properties based upon the specified standard.

Command Syntax: | [:SENSe]:DDEMod[:FORMat]:PRESet <standard>
<standard> | ::= | "Nadc" | "Gsm" | "Dect" | "CdmaBaseStation" | "CdmaMobileTerminal" | "Pdc" | "Php" | "Phs" | "Cdpd" | "Tetra" | "Apco" | "Dtv8" | "Dtv16" | "Dvb16" | "Dvb32" | "Dvb64" | "Edge" | "Bluetooth" | "Ieee80211B" | "HiperlanLowBitrate" | "HiperlanHighBitrate" | "Wcdma" | "Vdl3" | "Zigbee868" | "Zigbee915" | "Zigbee2450" | "DvbApsk16CodingRateTwoThirds" | "DvbApsk16CodingRateThreeFourths" | "DvbApsk16CodingRateFourFifths" | "DvbApsk16CodingRateFiveSixths" | "DvbApsk16CodingRateEightNinths" | "DvbApsk16CodingRateNineTenths" | "DvbApsk32CodingRateThreeFourths" | "DvbApsk32CodingRateFourFifths" | "DvbApsk32CodingRateFiveSixths" | "DvbApsk32CodingRateEightNinths" | "DvbApsk32CodingRateNineTenths" | "Dvb128" | "Dvb256" | "MilStd188181CCpmOption21" | "Apco25Phase2HarmonizedCpm" | "Apco25Phase2HarmonizedDifferentialQpsk" | "DvbEuropeDocsisQam64" | "DvbEuropeDocsisQam256" | "DvbNorthAmericaDocsisQam64" | "DvbNorthAmericaDocsisQam256" | "DvbJapanIsdbcQam64" | "ShapedOffsetQpskTGIrig10604" | "Wisun2Fsk50KbpsIndexOne" | "Wisun2Fsk100KbpsIndexOne" | "Wisun2Fsk100KbpsIndexOneHalf" | "Wisun2Fsk150KbpsIndexOneHalf" | "Wisun2Fsk200KbpsIndexOne" | "Wisun2Fsk200KbpsIndexOneHalf" | "Wisun2Fsk300KbpsIndexOneHalf"
Remarks: | <none>
Example: |
    :DDEM:PRES "Nadc"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.MeasurementExtension.Preset Agilent.SA.Vsa.DigitalDemod.Standard

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |