[:SENSe]:W11A:ADVanced:SYNC:REFerence | command/query

Gets or sets which part of the burst preamble to use as reference for initial timing synchronization.

Command Syntax: | [:SENSe]:W11A:ADVanced:SYNC:REFerence <value>
<value> | ::= | "ShortTraining" | "ChannelEstimation"
Query Syntax: | [:SENSe]:W11A:ADVanced:SYNC:REFerence?
Returns | ::= | "ShortTraining" | "ChannelEstimation"
Remarks: | <none>
Example: |
    :W11A:ADV:SYNC:REF "ShortTraining"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211Agjp.Interfaces.MeasurementExtension.SynchronizationReference Agilent.SA.Vsa.Wlan80211Agjp.SynchronizationReference

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |