[:SENSe]:LTE[:FORMat]:TDD:ULDLconfig | command/query

Gets or sets the Uplink/Downlink configuration type for TDD.

Command Syntax: | [:SENSe]:LTE[:FORMat]:TDD:ULDLconfig <value>
<value> | ::= | "Allocation0" | "Allocation1" | "Allocation2" | "Allocation3" | "Allocation4" | "Allocation5" | "Allocation6"
Query Syntax: | [:SENSe]:LTE[:FORMat]:TDD:ULDLconfig?
Returns | ::= | "Allocation0" | "Allocation1" | "Allocation2" | "Allocation3" | "Allocation4" | "Allocation5" | "Allocation6"
Remarks: | <none>
Example: |
    :LTE:TDD:ULDL "Allocation0"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.UplinkDownlinkAllocation Agilent.SA.Vsa.Lte.UplinkDownlinkAllocationType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |