:INPut:ANALog:RANGe:LIST | command/query

Gets/sets the input range (in Vpk) of multiple input channels.

Command Syntax: | :INPut:ANALog:RANGe:LIST <rangeBaseUnits>
<rangeBaseUnits> | ::= | Comma separated values of Real number
Query Syntax: | :INPut:ANALog:RANGe:LIST?
Returns | ::= | Comma separated values of Real number
Remarks: | <none>
Example: |
    // Set the range to 10 Vpk on the 1st channel and 1 Vpk on the 2nd
    :INP:ANAL:RANG:LIST 10.0,1.0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.AnalogChannel.Range

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |