[:SENSe]:LTE:DECode:PDSCh | command/query

Gets or sets the PDSCH Bit Vector Selection to be applied.

Command Syntax: | [:SENSe]:LTE:DECode:PDSCh <value>
<value> | ::= | "Mapped" | "Descrambled" | "DeRateMatched" | "DecodedCB" | "DecodedTB"
Query Syntax: | [:SENSe]:LTE:DECode:PDSCh?
Returns | ::= | "Mapped" | "Descrambled" | "DeRateMatched" | "DecodedCB" | "DecodedTB"
Remarks: | <none>
Example: |
    :LTE:DEC:PDSC "Mapped"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.PdschBitVectorSelect Agilent.SA.Vsa.Lte.PdschBitVectorSelectType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |