# Build_0061 completed at Tue May 21 17:47:31 PDT 2013 on firma
# These build_notes were derived from adm/build_notes.txt
# 
 
 Knute Kresie (KK) writes about this Smart3plus Firmware build (Build_0061):
                                          
    ===============================
    SUMMARY: This firmware set is for 5973N/5973inert/Carrera/Sumo(5975)
             using SC3.2 or SC3+ or a SC3 having 36MB DSP DRAM.
             This is the first GCMS firmware Build fully compatible
             with SmartCard3.2 (SC3.2).

    This build was built using:
    1. the Subversion version control system, and do_build.ksh and
    2. a set of svn_* ksh scripts in my (knute) firma:$HOME/mybin
       mapped to $SVNREP/svn_misc/svn_remsh in the
       Subversion repository SVNREP=http://scssvn.scs.agilent.com/svn/GCMS, and
       "build tools and process" changes listed below.


    ===============================
    Regarding this build of MSSC.O:


    Modified mssc/mse73/src/config/hp7up.c

   08May2013 KK  Revise reporting of "hivacp" (HiVac Pressure) sensor values to
             enable MH GUI to show "Off" or "N/C"(not connected) or valid value
              as requested in TeamTrack LSCA Hardware Issue#16778.
              Added pressureConvertQuadRS232() and HiVacGaugeON()
              copied from mstonga (5977).
              For "Off" and "N/C" report -2.0 and -1.0 (existing) respectively.
              Revise reporting of "forpres" (Foreline Pressure, diff pump only)
              to increase fraction digits from 3 to 5 so that when CSUOM="kPa"
              the value reported to MH avoids loss of precision due to rounding
              (e.g. 0.00359 kPa instead of 0.004 kPa) per LSCA SW TT#200066.
              Similar change may be needed in WUI and LUI displays.



X   Modify   mssc/mse73/src/config/msConfig.c

X   PENDING: Derive 5975 code from 5977 msConfig.c to 
X            detect "Hw-FW MisMatch" and set IncompatibleMainBoardAbort=TRUE.
X            Also see slick/server.c.


X   Modify   mssc/common/src/sicl/siclSup.c

X   FUTURE:   Remove as much SICL-related code as possible without affecting
X             Slick or the MSSC parser operations and event handling.


X   Modify   mssc/mse73/src/prog/Psys.c

X   PENDING:  Consider using safer 5977 cpystrn() return from instStat7up().



    Modified mssc/mse73/src/init/rev.c

    21Feb2013 KK  Changed MSSC version to    "7.02.18"    (for Build_0060)
    08May2013 KK  Changed MSSC version to    "7.02.18A"
    21May2013 KK  Changed MSSC version to    "7.02.19"



X   =========================================================
X   Regarding the DSP (AE) component of this build of MSSC.O:
X   No changes since the previous build.


    ==============================
    Regarding this build of LUI.O:


    Modified lui/lui.c

    08May2013 KK  Modified showHighVacPressure() to show "Gauge is OFF"
              when "hivacp" (High Vacuum Pressure sensor) returns -2.0.
              Removed LUIhttp_get() and references to it. See NOTE.4
    08May2013 KK  Modified showForePress() to provide at least three
              significant digits of precision when CSUOM is "kPa" that is
              popular in Japan.  See LSCA Software TeamTrack issue#200066.


    LUI.O identification:

    This LUI displays user-visible Front Panel version "03.218A.20130508" and
    includes file version string "lui.c version 08May2013 19:22 . . .".
    This LUI requires MSSC 5.02.18A or greater.


X   ===============================
X   Regarding this build of httpd.o
X   No changes since the previous build.


X   =====================================
X   Regarding this build of wdsmall_run.o (WUI4MSD)
X   No changes since the previous build.

X   PENDING: Revise Instrument Control - CI page, CIPI Status
X            (Idle/Busy, ...) to start with (Run/Quit,Idle/Busy,...)
X            and better handling of that info when CIPI_NO_FCB_RESPONSE.



    =====================================
    Regarding this build of slick_run.o


    Modified  slick/server.c

    20May2013 KK  To remedy truncated PC hostname (LSCA HW TT#17815)
              modified SlickSessConServer() to correct wrong
              SlickChemStaHostName array size used near
              "Apparently same MassHunter wants to re-connect.".
              Changed version string to 7.06 .


X   Modify   slick/server.c
X   PENDING: Perhaps changes related to Slick SIMramp > 1000 points problem.


    ===================================
    Regarding the firmware build tools and process:


    Modified  adm/build_notes.txt  (this file).


X   ===================================================
X   Regarding the firmware installation tool (msupdate)
X   No changes since the previous build.

