Changes to 3.02.47
Change G6120B, G6130B and G6150B to fast polarity switching configuration.
July 25, 2013

Change from 3.02.48
Use 6 seconds fault mask period for both fast and slow power supply to avoid having temporary fault
Aug. 9, 2013
