Zigbee Module Examples

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Files
Communications Examples

## Files
file | example_basic_comms_coordinator_afzdo.c
| Resets Module, configures this device to be a Zigbee Coordinator, and displays any messages that are received. Uses the AF/ZDO interface.
file | example_basic_comms_coordinator_sapi.c
| Resets Module, configures this device to be a Zigbee Coordinator, and displays any messages that are received. Uses the Simple API.
file | example_basic_comms_end_device_afzdo.c
| Resets Radio, configures this device to be a Zigbee End Device, joins a network, then sends a message to the coordinator every few seconds. Sleeps inbetween transmissions. Will also transmit a message when the button is pressed.
file | example_basic_comms_router_afzdo.c
| Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator once per second. Uses the AF/ZDO interface. Pressing the button will display device information.
file | example_basic_comms_router_sapi.c
| Resets Radio, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator once per second. Uses the Simple API.
file | example_fragmentation_coordinator_afzdo.c
| Resets Module, configures this device to be a Zigbee Coordinator, and displays any messages that are received. If the message is extended then gets all the parts and displays it. Uses the AF/ZDO interface.
file | example_fragmentation_router_afzdo.c
| Resets Module, configures this device to be a Zigbee Router, joins a network, then sends an extended length message to the coordinator periodically. Uses the AF/ZDO interface. Pressing the button will display device information.
file | example_secure_comms_coordinator_afzdo.c
| Resets Radio, configures this device to be a Zigbee Coordinator, and displays any received messages. Supports several security options such as preconfigured key, etc. Uses the AF/ZDO interface.
file | example_secure_comms_router_afzdo.c
| Resets Radio, configures this device to be a Zigbee Router, joins a network, initializes security and then sends a message to the coordinator once per second. Uses the AF/ZDO interface.

## Detailed Description