Zigbee Module Examples

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Todo List

Global halSpiInit (unsigned char port, unsigned char baudRate)
  implement baudRate
Global setRfTestMode (uint8_t mode, uint8_t channel, uint8_t txPower, uint8_t txTone)
  refactor with void sysNvWrite(uint8_t nvItem, uint8_t* data) ?
Global toggleLed (unsigned char led)
  this should read from a globals file based on the type of device, how many LEDs, etc.
Global toggleLed (unsigned char led)
  this should read from a globals file based on the type of device, how many LEDs, etc.
Global waitForDeviceState (unsigned char expectedState, uint16_t timeoutMs)
  modify this if using UART.