Zigbee Module Examples

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

- File List
- Globals

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
example_hello_world.c File Reference
Hardware Driver Examples

Outputs "Hello World" to console and toggles LED approximately once per second. More...

`#include "../HAL/hal.h"`
`#include <stdint.h>`

## Functions
int | main (void)

## Detailed Description

Outputs "Hello World" to console and toggles LED approximately once per second.

Configures the debug console UART pins and LED pin accordingly; loops and outputs text.

If you aren't seeing the message:

- Verify that hardware is installed correctly: Open the Device Manager: Go to Start : Run... type in devmgmt.msc and press Return. Then click on the + symbol next to ports. Note the COM port number next to the ez430 board.
- Verify that your terminal program is configured correctly: If using HyperTerminal, open the Device Manager: Go to Start : Run... type in hypertrm.exe and press Return. We recommend TeraTerm, as it is much better.
- Verify that the COM port number is correct and the baud rate and other configuration is correct.
- Verify that the application is running - verify that LED is blinking.
- Verify that the application is outputting bytes on the serial port: Use an oscilloscope to probe the microcontroller's Tx pin and verify that the UART is working.
- Using the debugger, stop the processor and see where it stops. It normally should halt in SysCtlDelay().

Rev:
  1642

Author:
  dsmith

Date:
  2012-10-31 11:17:04 -0700 (Wed, 31 Oct 2012)

# Support

Please refer to the wiki at www.anaren.com/air-wiki-zigbee for more information. Additional support is available via email at the following addresses:

- Questions on how to use the product: AIR@a.nosp@m.nare.nosp@m.n.com
- Feature requests, comments, and improvements: featu.nosp@m.rere.nosp@m.quest.nosp@m.s@te.nosp@m.slaco.nosp@m.ntro.nosp@m.ls.co.nosp@m.m
- Consulting engagements: sales.nosp@m.@tes.nosp@m.lacon.nosp@m.trol.nosp@m.s.com

# License

Copyright (c) 2012 Tesla Controls. All rights reserved. This Software may only be used with an Anaren A2530E24AZ1, A2530E24CZ1, A2530R24AZ1, or A2530R24CZ1 module. Redistribution and use in source and binary forms, with or without modification, are subject to the Software License Agreement in the file "anaren_eula.txt"

YOU FURTHER ACKNOWLEDGE AND AGREE THAT THE SOFTWARE AND DOCUMENTATION ARE PROVIDED “AS IS” WITHOUT WARRANTY OF ANY KIND, EITHER EXPRESS OR IMPLIED, INCLUDING WITHOUT LIMITATION, ANY WARRANTY OF MERCHANTABILITY, TITLE, NON-INFRINGEMENT AND FITNESS FOR A PARTICULAR PURPOSE. IN NO EVENT SHALL ANAREN MICROWAVE OR TESLA CONTROLS BE LIABLE OR OBLIGATED UNDER CONTRACT, NEGLIGENCE, STRICT LIABILITY, CONTRIBUTION, BREACH OF WARRANTY, OR OTHER LEGAL EQUITABLE THEORY ANY DIRECT OR INDIRECT DAMAGES OR EXPENSE INCLUDING BUT NOT LIMITED TO ANY INCIDENTAL, SPECIAL, INDIRECT, PUNITIVE OR CONSEQUENTIAL DAMAGES, LOST PROFITS OR LOST DATA, COST OF PROCUREMENT OF SUBSTITUTE GOODS, TECHNOLOGY, SERVICES, OR ANY CLAIMS BY THIRD PARTIES (INCLUDING BUT NOT LIMITED TO ANY DEFENSE THEREOF), OR OTHER SIMILAR COSTS.