Zigbee Module Examples

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Files
Hardware Driver Examples

## Files
file | example_button_interrupt.c
| Toggles LED0 when button pressed.
file | example_hello_world.c
| Outputs "Hello World" to console and toggles LED approximately once per second.
file | example_I2C_test.c
| tests the I2C interface
file | example_read_color_sensor.c
| Uses the MSP430's I2C interface to read the external color sensor.
file | example_read_eeprom.c
| reads and writes the EEPROM
file | example_read_IR_temperature_sensor.c
| Uses the I2C interface to read the external IR temperature sensor.
file | example_read_supply_voltage.c
| Uses the ADC to measure the supply voltage and toggles LED1 approximately once per second.
file | example_timer_interrupt.c
| Uses the microcontroller's internal oscillator to configure a timer to wake up periodically. Toggles LED0 when an interrupt is generated from the timer. Otherwise sleeps.

## Detailed Description