Zigbee Module Examples

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Files
Simple Applications

## Files
file | example_network_explorer.c
| Allows the user to configure this device as either a Coordinator, Router, or End device and explore various features of the Zigbee Module, such as sending messages via short address or long address, finding devices, etc. Uses the AF/ZDO interface. Uses a command line interface (CLI).
file | example_simple_application_coordinator_afzdo.c
| Resets Module, configures this device to be a Zigbee Coordinator, and displays any messages that are received. If the message contains a known object-identifier (OID) then parses the contents of the OID. Also displays received value to RGB LED and allows user to use the pushbutton to select which OID is displayed on the RGB LED.
file | example_simple_application_end_device_afzdo.c
| Resets Module, configures this device to be a Zigbee End Device, joins a network, then sends a message to the coordinator periodically with information from the peripherals.
file | example_simple_application_router_afzdo.c
| Resets Module, configures this device to be a Zigbee Router, joins a network, then sends a message to the coordinator periodically with information from the peripherals.

## Detailed Description