Zigbee Module Examples

- Main Page
- Related Pages
- Modules
- Data Structures
- Files

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Files
Module Interface Examples

## Files
file | example_get_mac_address.c
| Resets Module, gets MAC Address.
file | example_get_random.c
| Resets Radio, gets a random number using SYS_RANDOM command and displays it.
file | example_get_version.c
| Resets Radio, gets module version information using SYS_VERSION command and displays it.
file | example_measure_module_current.c
| Simple utility to demonstrate how to measure module current using onboard current sense amplifier. To generate sufficient current to measure we turn the module on and off using its RF Test functionality.
file | example_read_digital_io.c
| Resets Module, configures all four of the GPIO pins as inputs with pullups, then reads out the value of these pins to console once per second, between 0x00 (all low) to 0x0F (all high). To test, start this application then connect one or more GPIO pins to GND. You will see the value change accordingly.
file | example_read_nonvolatile_memory.c
| Resets Module, reads out the contents of all user non-volatile (NV) items and displays to console.
file | example_reset_module.c
| Resets Module, parses message received and displays to console.
file | example_rf_tester.c
| Simple utility to configure the Module to output an RF test signal.
file | example_write_digital_io.c
| Resets Module, configures all four of the GPIO pins as outputs, then toggles the GPIO pins once per second. To test, monitor GPIO pins with an oscilloscope.
file | example_write_nonvolatile_memory.c
| Resets Module, prompts the user for which NV item to write (1-6) and writes test data to that location.

## Detailed Description