12000A Operation Manual Addendum

List Mode Power Level 

Description:
Output levels exhibit unleveled performance while switching from one point to the next in list mode.

Firmware Version:
V0.73 B49-19 and higher. 

Correction:
Programming new lists should include a sequence that establishes the first point of a new list. The first point must be programmed for level. Frequency and dwell can be omitted. The list is cleared. Then the list can be programmed normally. The following is an example of the sequence to resolve the unleveled output condition:

LA 1,0
/*Add first point to list number 1*/

LL 1,1,15.0000 DM
/*Set first point level to 15 dBm. Level is not critical*/

LC 1
/*Clear list 1*/

