00000001:Chinese
00000002:English
00000003:Monitor Area
00000004:Filter Area
00000005:Enable
00000006:Disable
00000007:Target Area
00000008:Target Position
00000009:Serial Port:
0000000A:Baudrate:
0000000B:Open
0000000C:Close
0000000D:XY Axis
0000000E:X Axis(m):
0000000F:Y Axis(m):
00000010:Set Up
00000011:Target Show
00000012:Area Setting
00000013:Area No:
00000014:Area Status:
00000015:Area Type:
00000016:Area Position
00000017:Start(X,Y):
00000018:End(X,Y):
00000019:Mouse Select
0000001A:Cancel All Area
0000001B:Target Area
0000001C:Serial Port Setting
0000001D:Language:
0000001E:To set the radar baudrate to：%1?
0000001F:Tips
00000020:The software will be rebooted,sure to switch the language?
00000021:The radar baudrate setup successful!
00000022:The radar baudrate setup failed!
00000023:The value of the start point X  was out the range[-8.0, 8.0]
00000024:The value of the end point X was out the range[-8.0, 8.0]
00000025:The value of the start point Y was out the range[0.0, 8.0]
00000026:The value of the end point Y was out the range[0.0, 8.0]
00000027:The baudrate of the opened serial is wrong!