[:SENSe]:MBOFdm:ADVanced:FREQhop | command/query

Gets or sets the frequency hopping analysis type.

Command Syntax: | [:SENSe]:MBOFdm:ADVanced:FREQhop <value>
<value> | ::= | "Hopped" | "NotHopped" | "ForceFfi"
Query Syntax: | [:SENSe]:MBOFdm:ADVanced:FREQhop?
Returns | ::= | "Hopped" | "NotHopped" | "ForceFfi"
Remarks: | <none>
Example: |
    :MBOF:ADV:FREQ "Hopped"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.MBOfdm.Interfaces.MeasurementExtension.FrequencyHopAnalysis Agilent.SA.Vsa.MBOfdm.FrequencyHopAnalysisType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |