[:SENSe]:LTE:PROFile:PDCCh:ALLocation | command/query

Gets or sets the 10 allocation subframes for PDCCH allocations.

Command Syntax: | [:SENSe]:LTE:PROFile:PDCCh:ALLocation <symbolsPerSubframe>
<symbolsPerSubframe> | ::= | Comma separated values of Integer number
Query Syntax: | [:SENSe]:LTE:PROFile:PDCCh:ALLocation?
Returns | ::= | Comma separated values of Integer number
Remarks: | <none>
Example: |
    :LTE:PROF:PDCCh:ALLocation 1,2,1,2,1,2,1,2,1,1
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.SetPdcchAllocation

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |