[:SENSe]:C2K:CHANnel:IQBRanch | command/query

Gets or sets the branch of the reverse code channel to use for displaying symbol bits.

Command Syntax: | [:SENSe]:C2K:CHANnel:IQBRanch <value>
<value> | ::= | "I" | "Q"
Query Syntax: | [:SENSe]:C2K:CHANnel:IQBRanch?
Returns | ::= | "I" | "Q"
Remarks: | <none>
Example: |
    :C2K:CHAN:IQBR "I"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Cdma2000.Interfaces.MeasurementExtension.IQBranch Agilent.SA.Vsa.Cdma2000.IQBranch

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |