[:SENSe]:RFID:SYNCsearch:PATTern | command/query

Gets or sets the pattern used by sync search when the synchronization search type is a standard pattern.

Command Syntax: | [:SENSe]:RFID:SYNCsearch:PATTern <value>
<value> | ::= | "Iso1800004Mode1ForwardPreamble" | "Iso1800004Mode1ForwardStartDelimiter1" | "Iso1800004Mode1ReturnPreamble" | "Iso1800006AForwardSof" | "Iso1800006AForwardEof" | "Iso1800006AReturnPreamble" | "Iso1800006BForwardPreamble" | "Iso1800006BForwardStartDelimiter1" | "Iso1800006BForwardStartDelimiter2" | "Iso1800006BForwardStartDelimiter3" | "Iso1800006BForwardStartDelimiter4" | "Iso1800006BReturnPreamble" | "EpcC1G2ForwardPreamble" | "EpcC1G2ForwardFrameSync" | "EpcC1G2ForwardRTCal" | "EpcC1G2ForwardTRCal" | "EpcC1G2ReturnFM0PreambleTRext0" | "EpcC1G2ReturnFM0PreambleTRext1" | "EpcC1G2ReturnMillerPreambleTRext0" | "EpcC1G2ReturnMillerPreambleTRext1"
Query Syntax: | [:SENSe]:RFID:SYNCsearch:PATTern?
Returns | ::= | "Iso1800004Mode1ForwardPreamble" | "Iso1800004Mode1ForwardStartDelimiter1" | "Iso1800004Mode1ReturnPreamble" | "Iso1800006AForwardSof" | "Iso1800006AForwardEof" | "Iso1800006AReturnPreamble" | "Iso1800006BForwardPreamble" | "Iso1800006BForwardStartDelimiter1" | "Iso1800006BForwardStartDelimiter2" | "Iso1800006BForwardStartDelimiter3" | "Iso1800006BForwardStartDelimiter4" | "Iso1800006BReturnPreamble" | "EpcC1G2ForwardPreamble" | "EpcC1G2ForwardFrameSync" | "EpcC1G2ForwardRTCal" | "EpcC1G2ForwardTRCal" | "EpcC1G2ReturnFM0PreambleTRext0" | "EpcC1G2ReturnFM0PreambleTRext1" | "EpcC1G2ReturnMillerPreambleTRext0" | "EpcC1G2ReturnMillerPreambleTRext1"
Remarks: | <none>
Example: |
    :RFID:SYNC:PATT "Iso1800004Mode1ForwardPreamble"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Rfid.Interfaces.MeasurementExtension.SynchronizationSearchStandardPattern Agilent.SA.Vsa.Rfid.StandardSynchronizationPattern

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |