[:SENSe]:EVDO:CHANnel:FACHannel | command/query

Gets or sets the active channel in the forward link direction.

Command Syntax: | [:SENSe]:EVDO:CHANnel:FACHannel <value>
<value> | ::= | "None" | "Data"
Query Syntax: | [:SENSe]:EVDO:CHANnel:FACHannel?
Returns | ::= | "None" | "Data"
Remarks: | <none>
Example: |
    :EVDO:CHAN:FACH "None"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Cdma1xEvdo.Interfaces.MeasurementExtension.ForwardActiveChannel Agilent.SA.Vsa.Cdma1xEvdo.ForwardActiveChannelType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |