[:SENSe]:MBOFdm:ADVanced:TONE:NULLing:THReshold | command/query

Gets or sets the tone nulling threshold (in dB).

Command Syntax: | [:SENSe]:MBOFdm:ADVanced:TONE:NULLing:THReshold <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:MBOFdm:ADVanced:TONE:NULLing:THReshold?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.MBOfdm.Interfaces.MeasurementExtension.ToneNullingThreshold

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |