[:SENSe]:C2K:PCHannel:ENABled | command/query

Gets or sets a value indicating whether to add predefined channels to gated active channel detection.

Command Syntax: | [:SENSe]:C2K:PCHannel:ENABled <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:C2K:PCHannel:ENABled?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :C2K:PCH:ENAB 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Cdma2000.Interfaces.MeasurementExtension.IsPredefinedCodeChannelsEnabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |