[:SENSe]:DDEMod:FILTer:REFerence:OQPSk:HSINe | command/query

Gets or sets a value indicating whether the user-defined reference filter for Offset QPSK uses Half-Sine pulse shaping.

Command Syntax: | [:SENSe]:DDEMod:FILTer:REFerence:OQPSk:HSINe <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:DDEMod:FILTer:REFerence:OQPSk:HSINe?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :DDEM:FILT:REF:OQPS:HSIN 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.MeasurementExtension.IsUserReferenceFilterLikeHalfSine

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |