[:SENSe]:ADEMod:STYLe | command/query

Gets or sets the type of analog demodulation to perform for this input channel.

Command Syntax: | [:SENSe]:ADEMod[1:N]:STYLe <demodType>
<demodType> | ::= | AM | FM | PM
Query Syntax: | [:SENSe]:ADEMod[1:N]:STYLe?
Returns | ::= | AM | FM | PM
Remarks: | <none>
Example: |
    :ADEM:STYL AM
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.AnalogDemod.Interfaces.AnalogDemodChannel.DemodStyle

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |