[:SENSe]:MBOFdm[:FORMat]:TFCode | command/query

Gets or sets the time frequency code. Ignored if time frequency code is auto-detected.

Command Syntax: | [:SENSe]:MBOFdm[:FORMat]:TFCode <value>
<value> | ::= | "Tfc1" | "Tfc2" | "Tfc3" | "Tfc4" | "Tfc5" | "Tfc6" | "Tfc7" | "Tfc8" | "Tfc9" | "Tfc10"
Query Syntax: | [:SENSe]:MBOFdm[:FORMat]:TFCode?
Returns | ::= | "Tfc1" | "Tfc2" | "Tfc3" | "Tfc4" | "Tfc5" | "Tfc6" | "Tfc7" | "Tfc8" | "Tfc9" | "Tfc10"
Remarks: | <none>
Example: |
    :MBOF:TFC "Tfc1"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.MBOfdm.Interfaces.MeasurementExtension.TimeFrequencyCode Agilent.SA.Vsa.MBOfdm.TfcType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |