[:SENSe]:W16E:TIME:REGion:PREDemod | command/query

Gets or sets what is displayed in the pre-demod time trace.

Command Syntax: | [:SENSe]:W16E:TIME:REGion:PREDemod <value>
<value> | ::= | "Frame" | "Zone" | "MeasurementInterval" | "Preamble"
Query Syntax: | [:SENSe]:W16E:TIME:REGion:PREDemod?
Returns | ::= | "Frame" | "Zone" | "MeasurementInterval" | "Preamble"
Remarks: | <none>
Example: |
    :W16E:TIME:REG:PRED "Frame"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Ieee80216Ofdma.Interfaces.MeasurementExtension.PreDemodRegion Agilent.SA.Vsa.Ieee80216Ofdma.PreDemodRegionType

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |