:INITiate:SANalyzer:DISConnect | command

Pauses all measurements associated with this hardware and disconnects from the hardware.

Command Syntax: | :INITiate:SANalyzer:DISConnect
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.HardwareConfiguration.Disconnect

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |