[:SENSe]:RFID:ADVanced:DISPlay:OFFamplitude:PERCent | command/query

Gets or sets a value indicating whether Off Amplitude in the Summary table trace is displayed in terms of percent.

Command Syntax: | [:SENSe]:RFID:ADVanced:DISPlay:OFFamplitude:PERCent <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:RFID:ADVanced:DISPlay:OFFamplitude:PERCent?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :RFID:ADV:DISP:OFF:PERC 0
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Rfid.Interfaces.MeasurementExtension.IsDisplayOffAmplitudeInPercent

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |