:INPut:TRIGger:FMASk:ACTive | command/query

Gets or sets which of the upper or lower masks to use.

Command Syntax: | :INPut:TRIGger:FMASk:ACTive <value>
<value> | ::= | "Upper" | "Lower" | "Both"
Query Syntax: | :INPut:TRIGger:FMASk:ACTive?
Returns | ::= | "Upper" | "Lower" | "Both"
Remarks: | <none>
Example: |
    :INP:TRIG:FMAS:ACT "Upper"
Version: | 17.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.FrequencyMaskTrigger.MaskToUse Agilent.SA.Vsa.FrequencyMaskTriggerMask

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |