[:SENSe]:INPut:CORRection:CONStant:DELay | command/query

Gets or sets the time delay added (in Sec) to the specified input channel.

Command Syntax: | [:SENSe]:INPut:CORRection[1:N]:CONStant:DELay <delay>
<delay> | ::= | Real number
Query Syntax: | [:SENSe]:INPut:CORRection[1:N]:CONStant:DELay?
Returns | ::= | Real number
Remarks: | <none>
Version: | 16.20 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.InputCorrection.Delay

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |