[:SENSe]:LTE:PROFile:MBSFn:PMCH:SCALefactor | command/query

Gets or sets the 10 subcarrier PMCH scale factors in dB

Command Syntax: | [:SENSe]:LTE:PROFile:MBSFn:PMCH:SCALefactor <scaleFactors>
<scaleFactors> | ::= | Comma separated values of Real number
Query Syntax: | [:SENSe]:LTE:PROFile:MBSFn:PMCH:SCALefactor?
Returns | ::= | Comma separated values of Real number
Remarks: | <none>
Example: |
    :LTE:PROF:MBSF:PMCH:SCAL 1,2,1,2,1,2,1,2,1,1
Version: | 16.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.MeasurementExtension.SetPmchScaleFactor

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |