:INPut:ANALog:CONNection | command/query

Gets or sets the input connection type (Single Ended or Differential).

Command Syntax: | :INPut:ANALog:CONNection <connection>
<connection> | ::= | SING | DIFF
Query Syntax: | :INPut:ANALog:CONNection?
Returns | ::= | SING | DIFF
Remarks: | <none>
Example: |
    :INP:ANAL:CONN SING
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Analog.Connection

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |