[:SENSe]:TDSCdma:CODE:SCRamble:GROuped | command/query

Gets or sets a value indicating whether the scramble code is restricted to the code group specified by downlink pilot code.

Command Syntax: | [:SENSe]:TDSCdma:CODE:SCRamble:GROuped <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:TDSCdma:CODE:SCRamble:GROuped?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :TDSC:CODE:SCR:GRO 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Tdscdma.Interfaces.MeasurementExtension.IsScrambleCodeGrouped

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |