[:SENSe]:W11A:ADVanced:EQUalizer:TRAining | command/query

Gets or sets the types of subcarriers used for training the equalizer.

Command Syntax: | [:SENSe]:W11A:ADVanced:EQUalizer:TRAining <value>
<value> | ::= | "Preamble" | "PreambleData"
Query Syntax: | [:SENSe]:W11A:ADVanced:EQUalizer:TRAining?
Returns | ::= | "Preamble" | "PreambleData"
Remarks: | <none>
Example: |
    :W11A:ADV:EQU:TRA "Preamble"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211Agjp.Interfaces.MeasurementExtension.EqualizerTraining Agilent.SA.Vsa.Wlan80211Agjp.EqualizerTraining

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |