[:SENSe]:DDEMod:COMPensate:MIRRor[:FREQuency] | command/query

Gets or sets a value indicating whether modulation analysis will mirror the frequency spectrum.

Command Syntax: | [:SENSe]:DDEMod:COMPensate:MIRRor[:FREQuency] <value>
<value> | ::= | 0 | 1
Query Syntax: | [:SENSe]:DDEMod:COMPensate:MIRRor[:FREQuency]?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :DDEM:COMP:MIRR 0
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.MeasurementExtension.IsFrequencyMirrored

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |