:TRACe:MARKer:BANDwidth:CALCulate | command/query

Gets or sets the Band Power summation method (either mean or RMS).

Command Syntax: | :TRACe[1:N]:MARKer[1:N]:BANDwidth:CALCulate <bandCalc>
<bandCalc> | ::= | "Mean" | "Rms"
Query Syntax: | :TRACe[1:N]:MARKer[1:N]:BANDwidth:CALCulate?
Returns | ::= | "Mean" | "Rms"
Remarks: | <none>
Example: |
    :TRAC:MARK:BAND:CALC "Mean"
Version: | 13.01 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Marker.BandCalc Agilent.SA.Vsa.MarkerBandCalc

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |