:INPut:TRIGger:FMASk:REFerence:STYLe:AMPLitude | command/query

Gets or sets the reference style to use for mask amplitudes.

Command Syntax: | :INPut:TRIGger:FMASk:REFerence:STYLe:AMPLitude <value>
<value> | ::= | "Range" | "Absolute"
Query Syntax: | :INPut:TRIGger:FMASk:REFerence:STYLe:AMPLitude?
Returns | ::= | "Range" | "Absolute"
Remarks: | <none>
Example: |
    :INP:TRIG:FMAS:REF:STYL:AMPL "Range"
Version: | 17.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.FrequencyMaskTrigger.AmplitudeReferenceStyle Agilent.SA.Vsa.FrequencyMaskTriggerAmplitudeReference

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |