[:SENSe]:W11N:ADVanced:SUBCarrier:NUMBer | command/query

Gets or sets which subcarrier to analyze (meaningful only if looking at a single subcarrier).

Command Syntax: | [:SENSe]:W11N:ADVanced:SUBCarrier:NUMBer <value>
<value> | ::= | Integer number
Query Syntax: | [:SENSe]:W11N:ADVanced:SUBCarrier:NUMBer?
Returns | ::= | Integer number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wlan80211N.Interfaces.MeasurementExtension.SubcarrierNumber

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |