[:SENSe]:LTE:PROFile:DLINk:USER:CW0:ENABled | command/query

Gets or sets a value indicating whether or not CW0 is allocated to the DL user

Command Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:CW0:ENABled <enabled>
<enabled> | ::= | 0 | 1
Query Syntax: | [:SENSe]:LTE:PROFile:DLINk:USER[1:N]:CW0:ENABled?
Returns | ::= | 0 | 1
Remarks: | <none>
Example: |
    :LTE:PROF:DLIN:USER:CW0:ENAB 0
Version: | 14.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Lte.Interfaces.DownlinkUser.IsCW0Enabled

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |