[:SENSe]:WCDMa:CHANnel:DESPread:ULINk:DECode | command/query

Gets or sets the despread channel type to assume for decoding.

Command Syntax: | [:SENSe]:WCDMa:CHANnel:DESPread:ULINk:DECode <value>
<value> | ::= | "None" | "Edpcch" | "HsdpcchSiso" | "HsdpcchMimoA" | "HsdpcchMimoB" | "HsdpcchDualCell"
Query Syntax: | [:SENSe]:WCDMa:CHANnel:DESPread:ULINk:DECode?
Returns | ::= | "None" | "Edpcch" | "HsdpcchSiso" | "HsdpcchMimoA" | "HsdpcchMimoB" | "HsdpcchDualCell"
Remarks: | <none>
Example: |
    :WCDM:CHAN:DESP:ULIN:DEC "None"
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Wcdma.Interfaces.MeasurementExtension.DespreadDecodeMode Agilent.SA.Vsa.Wcdma.DespreadDecodeMode

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |