[:SENSe]:DDEMod:FILTer:ABT | command/query

Gets or sets the α (alpha) or BT (bandwidth time product) parameter for measurement and reference filters.

Command Syntax: | [:SENSe]:DDEMod:FILTer:ABT <value>
<value> | ::= | Real number
Query Syntax: | [:SENSe]:DDEMod:FILTer:ABT?
Returns | ::= | Real number
Remarks: | <none>
Version: | 13.00 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.DigitalDemod.Interfaces.MeasurementExtension.FilterAlphaBT

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |