[:SENSe]:CORRection:ECONverter:SPECtrum | command/query

Gets or sets how the external frequency converter inverts (mirrors) the spectrum around the center frequency.

Command Syntax: | [:SENSe]:CORRection[1:N]:ECONverter:SPECtrum <value>
<value> | ::= | "Normal" | "Inverted"
Query Syntax: | [:SENSe]:CORRection[1:N]:ECONverter:SPECtrum?
Returns | ::= | "Normal" | "Inverted"
Remarks: | <none>
Example: |
    :CORR:ECON:SPEC "Normal"
Version: | 16.20 or later
.NET Equivalent: | For more operation and usage information, see: Agilent.SA.Vsa.Interfaces.Correction.ExternalConverterSpectrum Agilent.SA.Vsa.SpectralOrder

17.00

Copyright © 2000-2013 Agilent Technologies, Inc. |